**1.5-1.8T**

## **叉车规格**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| General | 1 | Model | | |  | FD15T-M2WC3 | FD18T-M2WC3 |
| 2 | Optional Type | | |  | G(6)3 | |
| 3 | Power type | | |  | Diesel | |
| 4 | Rated capacity | | | kg | 1500 | 1800 |
| 5 | Load centre | | | mm | 500 | |
| Characteristic　&Dimension | 6 | Lift height | | | mm | 3000 | 3000 |
| 7 | Free lift height | | | mm | 135 | |
| 8 | Fork size | | LxWxT | mm | 920x100x35 | 920x100x35 |
| 9 | Fork regulating range | | Min./Max. | mm | 200/890 | |
| 10 | Mast tilt angle | | F/R | Deg | 6°/12° | |
| 11 | Front overhang | | | mm | 400 | |
| 12 | Rear overhang | | | mm | 465 | 510 |
| 13 | Min. ground clearance(Bottom of mast) | | | mm | 130 | |
| 14 | Overall dimensions | | Length to face of fork (without fork) | mm | 2255 | 2300 |
| 15 | Overall width | mm | 1070 | |
| 16 | Mast lowered height | mm | 2015 | |
| 17 | Mast extended height (with backrest) | mm | 3984 | |
| 18 | Overhead guard height | mm | 2110 | |
| 19 | Turning radius(outside) | | | mm | 2040 | 2075 |
| 20 | Min. right angle stacking aisle width (add load length and clearance) | | | mm | 1825 | 1857 |
| Performance | 21 | Speed | | Travel(Unladen) | km/h | 14.5 | |
| 22 | Lifting(Laden) | mm/s | 550(WC3) | |
| 23 | Lowering(Laden) | mm/s | 450 | |
| 24 | Max. Drawbar pull(Laden/unladen) | | | KN | 18/16(WC3) | |
|  | |
| 25 | Max. Gradeability(Laden) | | | % | 20 | |
| Chassis | 26 | Tyre | | Front |  | 6.50-10-10PR | |
| 27 | Rear |  | 5.00-8-8 PR | |
| 28 | Tread | | Front | mm | 890 | |
| 29 | Rear | mm | 920 | |
| 30 | Wheelbase | | | mm | 1400 | |
| Weight | 31 | Self weight | | | kg | 2590 | 2800 |
| 32 | Weight Distribution | Laden | Front Axle | kg | 3520 | 3950 |
| 33 | Rear Axle | kg | 570 | 650 |
| 34 | Unladen | Front Axle | kg | 1160 | 1260 |
| 35 | Rear Axle | kg | 1430 | 1540 |
| Battery | 36 | Battery | Voltage/Capacity | | V/Ah | 12/90 | |
| Transmission | 37 | Transmission | Manufacture | |  | China | |
| 38 | Type | |  | Powershift | |
| 39 | Stage | F/R |  | 1月1日 | |
| 40 | Operating pressure(For attachments) | | | MPa | 14.5 | |